    		usleep.doc

    At some time when developping MBSE BBS I decided that background utilities
    did't need full speed to do their jobs. BBS utilities under DOS needed
    to run as fast as possible because you needed to bring the bbs down to run
    these programs and users couldn't login during that time.

    Starting with mball, the allfiles creator, I inserted code that does usleep(1)
    after each 5 processed files. The 1 microsecond is not really the time the
    program pauses, it's probably a lot longer. I think this depends on the
    hardware type, (Intel, Sparc, Alpha etc) how long Linux will really suspends
    executing the utility.

    The program speed downgrade at the development machine that mball needed was
    3 times the original exection time, while system loading stayed under 30%.
    At that time the development machine is an 486DX2-66 with a Seagate ST32151N
    SCSI harddisk.

    The extra usleep code is only active if you run these utils with the -quiet
    switch and when this is set in mbsetup. See menu 1->5.
    With this switch, the program is mostly run by cron. If you onmit
    this switch, this is probably when you start the program manually, it will
    then always run at full speed, no matter what the setting in mbsetup is.

    If you have a fast system or don't care that the performance of your system
    drops because of background processing, you can turn this future off with
    mbsetup in the global section. (menu 1->5).

    Remember, if you have a PII-400 MMX or so with IDE disks, you may still have
    performance problems and need to set that switch to yes. There is only one
    way to find out if you need it.

    Well, actually, I tested this on a Dell Latitude PII-266, setting the switch to
    yes gave better performance then no. Why? The CPU has more time for the slow
    IDE disk. With the slow switch on programs runs even faster then with the switch
    off.

    Michiel.

Go Back